rp ag Infill Steel Mate Panel With Copper New Brickand CMU Cladding = @ Ai Windows, North Flevation Gi) Bamaicny Openings, ‘ ; G) 7 | | z j pe Comer St Et Restoration Dwgs.R-1*7 See Exterior Restoration Dwgs, 2 ' t gy SY i ZZ SI YMA VV" W"- YmJ—= |" 5 _ I, ay IN ete ( {a creas: CACO MMe eee! wy ee Wy ebie Ole —— AS Tee | 4 r 's r [eo ] fa a— ' 609 | , fi z A t > or Zz - : - Closet M ¥ t] Cree. YG cist: rf eal! eo Layers 5/8° Firecode “C | GWB on Metgl Furring SS SS SBCs | \ s Gan bool a WN (mv) bw SR — Nas SD SD ~ ae \ . t~— ~ SSS 2ey DAI Heor Ta" / @ Hicv.82-1 /e°= 2 yt 8 — yote I a W999 — _ vy r ae y. Lf ama 4 Ce REN om? ny SSS S =—— S ened RRS om N \ = SMOOogys_ LF ——— SS S35 On ae SN =_——— ia| 13) | MQ RQo0e IO 5 \N Existing Stone p be Res See Exterior Rewtoration SS DANS RQ SVG ¥§ > "4, SX RS N 4 TL MMU EE te Vii LLL SS WP hh > vhanical Drawings ! — — $$$ eee pe ai —_——_—_—_—$—$——_— —— EFTA00025136